{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","说明"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":8,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["监控设备编号","监控设备名称","回路表计地址","额定电压","额定电流","电流负载率门限","站点ID","电能质量分析"]
[1000000044,"测试导入功能设备44",1,0.6,3.4,0,1,"是"]
[1000000055,"测试导入功能设备55",1,0.6,3.4,0,1,"是"]

{"sheet":"说明","index":1,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["字段","是否必填","长度","描述"]
["监控设备编号","是",25,"自定义编码"]
["监控设备名称","是",50,"自定义名称"]
["回路表计地址","是",4,"默认值1"]
["额定电压","是","小数点保留3位","监控设备实际额定电压"]
["额定电流","是","小数点保留3位","根据监控设备容量、计算公式（容量/17.32）计算所得"]
["电流负载率门限","是","小数点保留3位","默认值0"]
["站点ID","是",10,"为站点对应自增唯一编号（请到对应站点页面获取或联系后台管理人员）"]
["电能质量分析","是",1,"值：是、否"]